We have a couple of questions regarding the MGS Trailing End Terminal as reported in TRP-03-279-13:

1. On pages 155 and 167, a single span rail (6’-3”), part a3 is incorporated into the design. Why? Is this necessary for the terminal to work properly?

2. On sheet 165, the cable anchor is shown to have an overall length of 80 inches. The old metric standard barrier guide calls out 2000 mm (78 ¾”). The old, old guide calls out 78 inches. Obviously some rounding was applied when it was made metric. This cable is not shown in the current on-line guide. Should this figure on page 165 really show 78 inches since it references a part number from the standard barrier guide, or does it require a special cable?